platformio device monitor --port COM3 --baud 115200

pio run --target uploadfs